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LINKVIL Hybrid DECT & Bluetooth Headset
LINKVIL DH602D Hybrid DECT & Bluetooth Headset is designed to meet demanding communication requirements across diverse work scenarios, delivering stable, smooth, and high-quality audio for professional collaboration environments. With dual-mode DECT and Bluetooth connectivity, users can switch seamlessly between computers, mobile phones, and IP phones to handle different communication needs with ease. The headset features advanced AI noise reduction and voice enhancement technology, supported by a three-microphone array, to ensure clear and natural voice transmission even in open offices or noisy environments. Smart wearing detection automatically identifies usage status to optimize call and media performance, while the two-sided visual busy light helps users stay focused and reduces interruptions. Its lightweight design and replaceable ear cushions improve wearing comfort, allowing for extended use without fatigue. DH602D enhances stability and efficiency in unified enterprise communication, making it a practical choice for modern offices and remote collaboration.
Highlights
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· Bluetooth 1-to-2 connection enables smoother switching between two Bluetooth devices.
· Pre-paired DT10 Dongle allows quick plug-and-play setup with PC or VoIP phone.
· Stable DECT wireless performance keeps users connected while moving around the office.
· Stereo audio with 3-Mic AI ENC enhances both listening clarity and voice pickup in busy offices.
· Replaceable ear cushions and battery support easier maintenance and longer business use.
Specifications
	DH602D Headset
	
	

	Microphone
	Type
	3 omnidirectional analog microphone

	
	Sensitivity
	-38±2 dBFS/Pa

	
	Frequency Range
	100Hz—10KHz

	Speaker
	Size
	φ32mm

	
	Max Input Power
	15mW

	
	Sensitivity
	102±3dB

	
	Frequency Range
	20Hz—20KHz

	
	Music Mode Bandwidth
	20Hz—20KHz

	
	Talk Mode Bandwidth
	100Hz—8KHz

	Audio
	Wearing Sensor
	Capacitive in-ear detection


Crystal sound experience
Full-duplex technology
	Feature	AI Environmental Noise Cancellation (AI ENC)
Acoustic Noise Reduction（ANS)
	
	
	Automatic Gain Control（AGC）

	
	User Hearing Protection
	EN50332

	Connectivity
	Device
	PC / Mobile Devices / VoIP Phone

	
	Method
	Bluetooth, DECT Dongle , USB Cable

	
	DECT Dongle Connection
	Headset Pairing

	
	DECT Wireless Range
	180m / 590 feet (Open area)

	
	DECT Frequency Bands
	1880—1900 MHz (EU); 1920—1930 MHz
(US/Canada)

	
	Secure DECT (level)
	Step C authentication-DSAA2, encryption-DSC2 (128 bit)

	
	Bluetooth Version
	5.3

	
	Bluetooth Profiles
	HFP, HSP, A2DP, SPP, AVRCP

	
	Bluetooth Range
	50m (Open area)

	
	Bluetooth Pairing List
	Up to 8 devices

	
	Simultaneous Bluetooth Connections
	2

	Compatibility
	Check Fanvil compatible list accordingly
	

	Battery
	Type
	Lithium Polymer Battery

	
	Battery Capacity
	600mAh

	
	Charging Time
	3h(5V/0.5A)

	
	Talk Time (DECT mode)
	12h

	
	Talk Time (Bluetooth mode)
	40h

	
	Music Time (DECT mode)
	12h

	
	Music Time (Bluetooth mode)
	54h

	
	Standby Time (DECT mode)
	92h

	
	Standby Time (Bluetooth mode)
	142h

	General
	Charging Method
	USB Cable

	
	Dimensions Gift-box
	215 x 196 x 85mm

	
	Dimensions Carton
	445 x415 x 235mm (10 PCS)

	
	Weight DH602 headset
	180g

	Carton Net weight
	2.2kg

	Carton Gross weight
	5.45kg

	Working temperature
	-10℃ to +60℃

	Storage temperature
	-20℃ to +70℃

	Working humidity
	10% to 95%RH


	Package Contents	DH602
Headset
DT10
DECT
Dongle
1.5-
meter
USB
Cable
Quick
Start
Guide

	
	Safety Information & Declaration

	Compliance
	




About LINKVIL
As a sub-brand of Fanvil, LINKVIL focuses on the research and development of A&V-IoT wireless communication products. Based on Audio & Video -IoT, LINKVIL helps customers to achieve full connection of wireless communication systems and will build a wireless communication Eco-system for multi-scenarios to help different industries accelerate their digital transformation.
Copyright
Copyright © 2026 Fanvil Link Technology Co., Ltd.
All rights reserved. No parts of this publication may be reproduced or transmitted in any form or by any means, electronic or mechanical, photocopying, recording, or otherwise, for any purpose, without the express written permission of Fanvil Link Technology Co., Ltd.
More Information
The above specifications may be updated in the future without prior notice. All hardware/software/physical features should be based on the final shipped products.
For more information, please visit: www.fanvil.com
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Web：www.fanvil.com
Tel: +86-755-2640-2199
E-mail: sales@fanvil.com Add:13th Floor, Building 2, Runzhi R&D Center, Xin'an Street, Bao'an District, Shenzhen, China
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